Exam
Name___________________________________

TRUE/FALSE.  Write 'T' if the statement is true and 'F' if the statement is false. 

1) 

The unit of measurement for conductance is the Coulomb.  

1) 

_______ 

2) 

Kilo equals 1,000 times the base unit.  

2) 

_______ 

3) 

Inductors store energy in an electrostatic field.  

3) 

_______ 

4) 

An electronic device which stores an electric charge is known as an inductor.  

4) 

_______ 

5) 

The symbol μ is an abbreviation for 10-6 or micro.  

5) 

_______ 

MULTIPLE CHOICE.  Choose the one alternative that best completes the statement or answers the question. 

6) 

Which of the following are common applications of electronics?  

6) 

_______ 

A) 

Consumer products  

B) 

Automation  

C) 

Computers  

D) 

Communications systems  

E) 

All of the above  

7) 

The symbol for Current is  

7) 

_______ 

A) 

A  

B) 

C  

C) 

I  

D) 

V  

8) 

The unit of measurement for current is the  

8) 

_______ 

A) 

Ohm  

B) 

Volt  

C) 

Ampere  

D) 

Watt  

9) 

The symbol for voltage is  

9) 

_______ 

A) 

A  

B) 

V  

C) 

R  

D) 

C  

10) 

The unit of measurement for voltage is the  

10) 

______ 

A) 

Ohm D 

B) 

Ampere  

C) 

Watt  

D) 

Volt  

11) 

The symbol for a resistor is  

11) 

______ 

A) 

C  

B) 

R  

C) 

V  

D) 

A  

12) 

The shortcut symbol for Ohms is  

12) 

______ 

A) 

. 

B) 

Ω 

C) 

α 

D) 

δ 

13) 

The unit of measurement for resistance is the  

13) 

______ 

A) 

Ohm  

B) 

Volt  

C) 

Watt  

D) 

Ampere  

14) 

Which of the following metric prefixes is NOT commonly used in electronics work?  

14) 

______ 

A) 

tera  

B) 

kilo  

C) 

milli  

D) 

micro  

E) 

pico  

15) 

Express the number 10,000 in proper scientific notation.  

15) 

______ 

A) 

10.0 × 103  

B) 

1.0 × 104  

C) 

1.0 × 103  

D) 

100.0 × 102  

16) 

Convert 4.7 mA to amperes.  

16) 

______ 

A) 

0.0047 A  

B) 

4,700 A  

C) 

47,000 A  

D) 

0.00047 A  

17) 

Convert 120 mW to W.  

17) 

______ 

A) 

0.00012 W  

B) 

0.12 W  

C) 

1,200 W  

D) 

120,000 W  

18) 

Convert 10,000 ohms to kΩ.  

18) 

______ 

A) 

1 kΩ 

B) 

1000 kΩ  

C) 

10 kΩ 

D) 

100 kΩ 

19) 

Convert 75 μV to mV.  

19) 

______ 

A) 

75,000 mV  

B) 

7500 mV  

C) 

0.000075 mV  

D) 

0.075 mV  

20) 

Convert 5.7 mW to μW.  

20) 

______ 

A) 

5,700 μW  

B) 

0.00057 μW  

C) 

0.057 μW  

D) 

57,000 μW  

21) 

Convert 6.8 × 10-5 W to the closest standard metric prefix.  

21) 

______ 

A) 

680 μW  

B) 

0.68 μW  

C) 

68 μW  

D) 

6.8 μW  

22) 

Convert 3.95 × 10-4 A to the closest standard metric prefix.  

22) 

______ 

A) 

39.5 mA  

B) 

395 mA  

C) 

0.395 mA  

D) 

3.95 mA  

Convert the following 

23) 

2 × 10-3 Amp = ________  

23) 

______ 

A) 

2 microamps  

B) 

2 amps  

C) 

0.5 milliamps  

D) 

2 milliamps  

24) 

4.7 kΩ = ________  

24) 

______ 

A) 

4.7 × 10-3 Ω  

B) 

4.7 × 10-4 Ω  

C) 

4.7 × 103 Ω  

D) 

47 × 10-3 Ω  

25) 

3.9 kΩ = ________  

25) 

______ 

A) 

39 × 10-3 Ω 

B) 

3.9 × 10-4 Ω  

C) 

3.9 × 105 Ω  

D) 

3.9 × 103 Ω  

26) 

980 microvolts = ________  

26) 

______ 

A) 

9.80 millivolts  

B) 

98 × 103 V  

C) 

980 × 10-3 V  

D) 

both A and C  

E) 

none of the above  

27) 

2.2 kV = ________  

27) 

______ 

A) 

2.2 × 10-4 V  

B) 

2,200 Volts  

C) 

2.2 × 10-3 V  

D) 

22 × 103 V  

28) 

Siemens is a unit for  

28) 

______ 

A) 

power  

B) 

resistance  

C) 

conductance  

D) 

voltage  

29) 

The shorthand method that uses a base number between 1 and 10 is called  

29) 

______ 

A) 

prefix  

B) 

engineering notation  

C) 

decimal  

D) 

scientific notation  

30) 

The symbol for power is  

30) 

______ 

A) 

W  

B) 

Q  

C) 

Z  

D) 

P  

31) 

Express 0.004730 = ________, ________.  

31) 

______ 

A) 

M473 × 103, .473 milli  

B) 

473 × 10-3, 4.73 milli  

C) 

4.73 × 10-3, 4.73 milli  

D) 

4.73 × 10-6, 4.73 micro  

32) 

Express 5.6 × 10-2 in milli, basic units, and micro.  

32) 

______ 

A) 

5600 milli, 56, 560 pico  

B) 

560 milli, 5.600, 5600 micro  

C) 

5.6 milli, 0.056, 56000 micro  

D) 

56 milli, 0.056, 56000 micro  

33) 

Multiply (99.2 × 10-6)(48 × 101) = ________, ________.  

33) 

______ 

A) 

4.76 × 10-4, 47.6 milli  

B) 

4.76 × 10-2, 47.6 milli  

C) 

476 × 10-3, 47.6 micro  

D) 

4.76 × 10-2, 47.6 nano  

34) 

Add (430 × 106) + (9.75 × 108) = ________, ________.  

34) 

______ 

A) 

14 × 109, 1.4 Giga  

B) 

1.4 × 109, 1.4 Giga  

C) 

1.4 × 109, 1.4 Mega  

D) 

14 × 109, 1.4 Giga  

35) 

Subtract (3462 × 100) - (2.22 × 102) = ________, ________.  

35) 

______ 

A) 

3.24 × 103, 3.24 kilo  

B) 

3.24 × 102, 3.24 kilo  

C) 

3.24 × 103, 3.24 milli  

D) 

3.24 × 104, 3.24 kilo  

36) 

Divide  =      

36) 

______ 

A) 

2.83 × 10-4, 283 micro  

B) 

2.83 × 10-2, 283 micro  

C) 

2.83 × 10-5, 283 micro  

D) 

2.83 × 10-3, 283 micro  

37) 

Convert 4,600,000 Ω to Mega Ω.  

37) 

______ 

A) 

4600 Mega Ω  

B) 

46 Mega Ω  

C) 

4.6 Mega Ω  

D) 

460 Mega Ω  

38) 

2 μF = ________ 

38) 

______ 

A) 

2000 nF  

B) 

200 pF  

C) 

2 × 10-6 F  

D) 

both A and C  

39) 

Express the number 51,000,000,000 in proper scientific notation.  

39) 

______ 

A) 

51 × 108  

B) 

5.1 × 109  

C) 

5.1 × 1011  

D) 

5.1 × 1010  

40) 

The SI system is  

40) 

______ 

A) 

based on a system of fundamental units 

B) 

an international system 

C) 

used for engineering work 

D) 

used for scientific work 

E) 

all of the above 

 

1) 

FALSE 

2) 

TRUE 

3) 

FALSE 

4) 

FALSE 

5) 

TRUE 

6) 

E 

7) 

C 

8) 

C 

9) 

B 

10) 

D 

11) 

B 

12) 

B 

13) 

A 

14) 

A 

15) 

B 

16) 

A 

17) 

B 

18) 

C 

19) 

D 

20) 

A 

21) 

C 

22) 

C 

23) 

D 

24) 

C 

25) 

D 

26) 

E 

27) 

B 

28) 

C 

29) 

D 

30) 

D 

31) 

C 

32) 

D 

33) 

B 

34) 

B 

35) 

A 

36) 

A 

37) 

C 

38) 

D 

39) 

D 

40) 

E